Description for the dataset
Geospatial Information Authority of Japan (2026)
## Description ##
	Description.docx
	Description of dataset (This document)

	term_of_use.txt
	Term of use for the dataset

	[Sub-beam 6]
	

	sb6_220606-260609_int.tif
	Wrapped LOS change [rad.]

	sb6_220606-260609_unw.tif
	Unwrapped LOS change [mm]

	sb6_220606-260609_lose.tif
	Map of LOS EW component

	sb6_220606-260609_losn.tif
	Map of LOS NS component

	sb6_220606-260609_cor.tif
	Map of normalized coherence

	[Sub-beam 7]
	

	sb7_220314-260609_int.tif
	Wrapped LOS change [rad.]

	sb7_220314-260609_unw.tif
	Unwrapped LOS change [mm]

	sb7_220314-260609_lose.tif
	Map of LOS EW component

	sb7_220314-260609_losn.tif
	Map of LOS NS component

	sb7_220314-260609_cor.tif
	Map of normalized coherence




## Summary of data ##
	Path
	023

	Orbit
	Descending

	Look direction
	Right

	Phase unwrapping
	Minimum cost flow (SNAPHU)



	
	Sub-beam 6
	Sub-beam 7

	Primary
	ALOS-2/PALSAR-2
2022.06.06
	ALOS-2/PALSAR-2
2022.03.14

	Secondary
	ALOS-4/PALSAR-3
2026.06.09
	ALOS-4/PALSAR-3
2026.06.09

	Mode
	SM3 (F6)
	SM3 (F7)

	Frame
	3480 – 3510
	3480 – 3500
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